FUJITSU|FUJITSU MAS3367NP 0103A|FUJITSU MAS3367NP 0103A-512:\
	:ty=fixed_rw_scsi:nc#27150:nt#4:ns#705:ss#512:rm#15000:\
	:fp#320:bp#0:ng#0:gs#0:ga#0:ao#0:\
	:os=mach_kernel:z0#64:z1:192:hn=mordor:ro=a:\
	:pa#63:sa#8388608:ba#8192:fa#1024:ca#4:da#4096:ra#10:oa=time:\
	:ia:ta=4.3BSD:aa:\
	:pb#8388671:sb#8388608:bb#8192:fb#1024:cb#4:db#4096:rb#10:ob=time:\
	:ib:tb=4.3BSD:ab:\
	:pc#16777279:sc#8388608:bc#8192:fc#1024:cc#4:dc#4096:rc#10:oc=time:\
	:ic:tc=4.3BSD:ac:\
	:pd#25165887:sd#8388608:bd#8192:fd#1024:cd#4:dd#4096:rd#10:od=time:\
	:id:td=4.3BSD:ad:\
	:pe#33554495:se#8388608:be#8192:fe#1024:ce#4:de#4096:re#10:oe=time:\
	:ie:te=4.3BSD:ae:\
	:pf#41943103:sf#8388608:bf#8192:ff#1024:cf#4:df#4096:rf#10:of=time:\
	:if:tf=4.3BSD:af:\
	:pg#50331711:sg#8388608:bg#8192:fg#1024:cg#4:dg#4096:rg#10:og=time:\
	:ig:tg=4.3BSD:ag:

May  4 01:29:47 mordor mach: NeXT Mach 4.2: Tue Jan 26 11:21:50 PST 1999; root(rcbuilder):Objects/mk-183.34.4.obj~2/RELEASE_I386
May  4 01:29:47 mordor mach: physical memory = 958.00 megabytes.
May  4 01:29:47 mordor mach: using 255 buffers containing 1.99 megabytes of memory
May  4 01:29:47 mordor mach: available memory = 943.61 megabytes. vm_page_free_count = 1d7ce
May  4 01:29:47 mordor mach: PCI Ver=2.10 BusCount=2 Features=[ BIOS16 CM1 SC1 ]
May  4 01:29:47 mordor mach: Found PCI 2.0 device: ID=0x06911106 at Dev=0 Func=0 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.0 device: ID=0x85981106 at Dev=1 Func=0 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.1 device: ID=0x06861106/0x00001106 at Dev=7 Func=0 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.0 device: ID=0x30571106 at Dev=7 Func=4 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.1 device: ID=0x87789004/0x78879004 at Dev=9 Func=0 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.1 device: ID=0x00351033/0x00351033 at Dev=10 Func=0 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.1 device: ID=0x00351033/0x00351033 at Dev=10 Func=1 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.0 device: ID=0x00091011 at Dev=11 Func=0 Bus=0
May  4 01:29:47 mordor mach: Found PCI 2.1 device: ID=0x0525102b/0x217d102b at Dev=0 Func=0 Bus=1
May  4 01:29:47 mordor mach: PCI bus support enabled
May  4 01:29:47 mordor mach: PnP: Plug and Play support enabled
May  4 01:29:47 mordor mach: PnP: Plug and Play BIOS present
May  4 01:29:47 mordor mach: PnP: read port 0x20b, max csn 1
May  4 01:29:47 mordor mach: PnP: csn 1: CTL00e4 s/n 0x1920ba48
May  4 01:29:47 mordor mach: ISA/EISA bus support enabled
May  4 01:29:47 mordor mach: ISA bus
May  4 01:29:47 mordor mach: DriverKit version 420
May  4 01:29:47 mordor mach: Registering: ISASerialPort0
May  4 01:29:47 mordor mach: ISASerialPort0: Base=0x03f8, IRQ=4, Type=16550AF/C/CF, FIFO=16
May  4 01:29:47 mordor mach: Registering: PS2Controller
May  4 01:29:47 mordor mach: Registering: PCKeyboard0
May  4 01:29:47 mordor mach: Registering: PCMCIA0
May  4 01:29:47 mordor mach: PCI bus support enabled
May  4 01:29:47 mordor mach: Registering: PCI0
May  4 01:29:47 mordor mach: Registering: EISA0
May  4 01:29:47 mordor mach: Registering: fc0
May  4 01:29:47 mordor mach: Registering: fd0
May  4 01:29:47 mordor mach: Adaptec 2940 Host Adapter found at Bus 0 Device 9
May  4 01:29:47 mordor mach: a2940_0: 16 Targets per Bus
May  4 01:29:47 mordor mach: Resetting SCSI Bus...
May  4 01:29:47 mordor mach: Registering: a2940_0 at 0xdc00
May  4 01:29:47 mordor mach: Registering: sc0 at a2940_0 SCSI Bus 0 Target 7
May  4 01:29:47 mordor mach: sd0: FUJITSU MAS3367NP 0103
May  4 01:29:47 mordor mach: Registering: sd0 at Target 0 LUN 0 at sc0
May  4 01:29:47 mordor mach: sd0: Device Block Size: 512 bytes
May  4 01:29:47 mordor mach: sd0: Device Capacity:   35068 MB
May  4 01:29:47 mordor mach: sd0: Disk Label:        Fujitsu
May  4 01:29:47 mordor mach: sd1: IBM-ESXS VPR036W3-ETS10FN S3C0
May  4 01:29:47 mordor mach: Registering: sd1 at Target 1 LUN 0 at sc0
May  4 01:29:47 mordor mach: sd1: Device Block Size: 512 bytes
May  4 01:29:47 mordor mach: sd1: Device Capacity:   34715 MB
May  4 01:29:47 mordor mach: sd1: Disk Label:        Backup
May  4 01:29:47 mordor mach: sd2: ZULUSCSI HARDDRIVE 2.0 
May  4 01:29:47 mordor mach: Registering: sd2 at Target 2 LUN 0 at sc0
May  4 01:29:47 mordor mach: sd2: No Valid Disk Label
May  4 01:29:47 mordor mach: sd2: Device Block Size: 512 bytes
May  4 01:29:47 mordor mach: sd2: Device Capacity:   2048 MB
May  4 01:29:47 mordor mach: sd3: IBM-ESXS VPR036W3-ETS10 1.0 
May  4 01:29:47 mordor mach: Registering: sd3 at Target 3 LUN 0 at sc0
May  4 01:29:47 mordor mach: sd3: Device Block Size: 512 bytes
May  4 01:29:47 mordor mach: sd3: Device Capacity:   34715 MB
May  4 01:29:47 mordor mach: sd3: Disk Label:        Zulu
May  4 01:29:47 mordor mach: sd4: HP DVD-ROM 305 1.01
May  4 01:29:47 mordor mach: Registering: sd4 at Target 6 LUN 0 at sc0
May  4 01:29:47 mordor mach: sd4: Waiting for drive to come ready..............
May  4 01:29:47 mordor mach: sd4: Disk Not Ready
May  4 01:29:47 mordor mach: Registering: sg0 at sc0
May  4 01:29:47 mordor mach: Registering: sg1 at sc0
May  4 01:29:47 mordor mach: Registering: sg2 at sc0
May  4 01:29:47 mordor mach: Registering: sg3 at sc0
May  4 01:29:47 mordor mach: Registering: event0
May  4 01:29:47 mordor mach: Registering: kmDevice0
May  4 01:29:47 mordor mach: rootdev 600, howto 0
May  4 01:29:47 mordor mach: Power management is enabled.
May  4 01:29:47 mordor mach: Registering: PS2Mouse
May  4 01:29:47 mordor mach: Registering: pp0
May  4 01:29:47 mordor mach: DECchip21140: PCI Dev: 11 Func: 0 Bus: 0
May  4 01:29:47 mordor mach: Registering: en0
May  4 01:29:47 mordor mach: DECchip21140 based adapter at port 0xe000 irq 11
May  4 01:29:47 mordor mach: DECchip21140 configured for 100BASE-TX (MII/SYM) interface
May  4 01:29:47 mordor mach: IP protocol enabled for interface en0, type "10MB Ethernet"
May  4 01:29:47 mordor mach: en0: Ethernet address 00:00:c0:af:8b:e4
May  4 01:29:47 mordor mach: MatroxMGA Driver v1.0
May  4 01:29:47 mordor mach: Copyright (c) 1999-2005 Mirko Viviani
May  4 01:29:47 mordor mach: 
May  4 01:29:47 mordor mach: Display: Mode selected: 1600 x 1200 @ 60 Hz (RGB:888/32)
May  4 01:29:47 mordor mach: Display0: Matrox Millennium G400 AGP
May  4 01:29:47 mordor mach: Display0: SGRAM size: 16 MB
May  4 01:29:47 mordor mach: Display0: RAMDAC: 300 MHz
May  4 01:29:47 mordor mach: Registering: Display0
May  4 01:29:47 mordor mach: PnP: configuring Creative SB AWE64  PnP Audio
May  4 01:29:47 mordor mach: SBSoundMidi: Sound Blaster SB32 (ver 4.0) at port 0x220.
May  4 01:29:47 mordor mach: SBSoundMidi at dma channels 1 and 5 irq 5
May  4 01:29:47 mordor mach: Registering: SBSoundMidi
May  4 01:29:47 mordor mach: SBSoundMidi: License found. Enabling driver.
May  4 01:30:00 mordor reboot: Reboot complete
May  4 01:30:02 mordor loginwindow[212]: Checking for DOS partitioned disk
May  4 01:30:10 mordor loginwindow[214]: netname look up success: NeXT 4.0 Pasteboard Server (1)
May  4 01:30:10 mordor loginwindow[214]: running /usr/lib/NextStep/Workspace.app/Workspace
May  4 01:30:10 mordor Workspace[214]: logged in

-bash-2.05b# ./Run
make all
Checking distribution of files
./pgms  exists
./src  exists
./testdir  exists
./doc  exists
./tmp  exists
./results  exists

         ############   #####        ## ############### ###############
         ############## #####        ## ############### ###############
         #####       ## #####        ##      #####      #####         
         #####       ## #####        ##      #####      #####         
         #####       ## #####        ##      #####      #####         
         ############   #####       ##       #####      ###############
         #############   ######### ##        #####      ###############
         #####       ##   ##########         #####      #####         
         #####       ##      #####           #####      #####         
         #####       ##      #####           #####      #####         
         #####       ##      #####           #####      #####         
         ##############      #####           #####      ###############
         ############        #####           #####      ###############

   #    #  #    #  #  #    #          #####   ######  #    #   ####   #    #
   #    #  ##   #  #   #  #           #    #  #       ##   #  #    #  #    #
   #    #  # #  #  #    ##            #####   #####   # #  #  #       ######
   #    #  #  # #  #    ##            #    #  #       #  # #  #       #    #
   #    #  #   ##  #   #  #           #    #  #       #   ##  #    #  #    #
    ####   #    #  #  #    #          #####   ######  #    #   ####   #    #

Dhrystone 2 without register variables  1 2 3 4 5 6

Dhrystone 2 using register variables  1 2 3 4 5 6

Arithmetic Test (type = arithoh)  1 2 3 4 5 6

Arithmetic Test (type = register)  1 2 3 4 5 6

Arithmetic Test (type = short)  1 2 3 4 5 6

Arithmetic Test (type = int)  1 2 3 4 5 6

Arithmetic Test (type = long)  1 2 3 4 5 6

Arithmetic Test (type = float)  1 2 3 4 5 6

Arithmetic Test (type = double)  1 2 3 4 5 6

System Call Overhead Test  1 2 3 4 5 6

Pipe Throughput Test  1 2 3 4 5 6

Pipe-based Context Switching Test  1 2 3 4 5 6

Process Creation Test  1 2 3 4 5 6

Execl Throughput Test  1 2 3 4 5 6

Filesystem Throughput Test (10 second test)  1 2 3 4 5 6
Filesystem Throughput Test (30 second test)  1 2 3 4 5 6

C Compiler Test  1 2 3

Shell scripts (1 concurrent)  1 2 3
Shell scripts (2 concurrent)  1 2 3
Shell scripts (4 concurrent)  1 2 3
Shell scripts (8 concurrent)  1 2 3

Dc: sqrt(2) to 99 decimal places  1 2 3 4 5 6

Recursion Test--Tower of Hanoi  1 2 3 4 5 6

==============================================================

  BYTE UNIX Benchmarks (Version 3.11)
  System -- mordor
  Start Benchmark Run: Thu May  4 01:47:07 PDT 2023
   1 interactive users.
Dhrystone 2 without register variables   2689256.5 lps   (10 secs, 6 samples)
Dhrystone 2 using register variables     2745889.0 lps   (10 secs, 6 samples)
Arithmetic Test (type = arithoh)         4419186.9 lps   (10 secs, 6 samples)
Arithmetic Test (type = register)        356012.9 lps   (10 secs, 6 samples)
Arithmetic Test (type = short)           215617.4 lps   (10 secs, 6 samples)
Arithmetic Test (type = int)             357971.6 lps   (10 secs, 6 samples)
Arithmetic Test (type = long)            357595.6 lps   (10 secs, 6 samples)
Arithmetic Test (type = float)           432840.1 lps   (10 secs, 6 samples)
Arithmetic Test (type = double)          432819.6 lps   (10 secs, 6 samples)
System Call Overhead Test                370368.6 lps   (10 secs, 6 samples)
Pipe Throughput Test                     392244.7 lps   (10 secs, 6 samples)
Pipe-based Context Switching Test        118803.6 lps   (10 secs, 6 samples)
Process Creation Test                      1888.6 lps   (10 secs, 6 samples)
Execl Throughput Test                      1417.1 lps   (9 secs, 6 samples)
File Read  (10 seconds)                  1081462.0 KBps  (10 secs, 6 samples)
File Write (10 seconds)                   17894.0 KBps  (10 secs, 6 samples)
File Copy  (10 seconds)                   13735.0 KBps  (10 secs, 6 samples)
File Read  (30 seconds)                  1085261.0 KBps  (30 secs, 6 samples)
File Write (30 seconds)                   17976.0 KBps  (30 secs, 6 samples)
File Copy  (30 seconds)                    9807.0 KBps  (30 secs, 6 samples)
C Compiler Test                             803.0 lpm   (60 secs, 3 samples)
Shell scripts (1 concurrent)               1344.3 lpm   (60 secs, 3 samples)
Shell scripts (2 concurrent)                753.0 lpm   (60 secs, 3 samples)
Shell scripts (4 concurrent)                383.3 lpm   (60 secs, 3 samples)
Shell scripts (8 concurrent)                190.0 lpm   (60 secs, 3 samples)
Dc: sqrt(2) to 99 decimal places          17227.0 lpm   (60 secs, 6 samples)
Recursion Test--Tower of Hanoi            33989.2 lps   (10 secs, 6 samples)

/Data/ByteBenchmark/pgms/index.base /tmp/25338.dat

                     INDEX VALUES            
TEST                                        BASELINE     RESULT      INDEX

Arithmetic Test (type = double)               2703.3   432819.6      160.1
Arithmetic Test (type = long)                 2827.0   357595.6      126.5
Arithmetic Test (type = register)             2847.5   356012.9      125.0
C Compiler Test                                 24.1      803.0       33.3
Dhrystone 2 without register variables       24179.3  2689256.5      111.2
Execl Throughput Test                           23.7     1417.1       59.8
File Copy  (30 seconds)                        518.0     9807.0       18.9
File Read  (30 seconds)                      18288.0  1085261.0       59.3
File Write (30 seconds)                        600.0    17976.0       30.0
Pipe-based Context Switching Test             1153.5   118803.6      103.0
Process Creation Test                           34.0     1888.6       55.5
Recursion Test--Tower of Hanoi                 323.8    33989.2      105.0
Shell scripts (8 concurrent)                     3.8      190.0       50.0
                                                                 =========
     SUM of 13 items                                                1037.7
     AVERAGE                                                          79.8

SCSI information for /dev/rsd0h
Drive type: FUJITSU MAS3367NP 0103A
512 bytes per sector
705 sectors per track
4 tracks per cylinder
27150 cylinder per volume (including spare cylinders)
168 spare sectors per cylinder
72 alternate tracks per volume
71819495 usable sectors on volume

Starting tests.
Line: time taken: 8245 ms, raw: 121.2856, factor: 15.1001
Curve: time taken: 4541 ms, raw: 220.2158, factor: 14.3495
Fill: time taken: 1935 ms, raw: 516.7959, factor: 16.3762
Transpose: time taken: 504 ms, raw: 1984.1270, factor: 132.1940
Composite: time taken: 24073 ms, raw: 41.5403, factor: 14.4992
Userpath: time taken: 31489 ms, raw: 31.7571, factor: 5.2591
Text: time taken: 3309 ms, raw: 302.2061, factor: 29.7198
Window move: time taken: 9656 ms, raw: 103.5626, factor: 4.4620
Window resize: time taken: 1777 ms, raw: 562.7462, factor: 13.9482
NXFactor = 27.323139
Tests complete, run time = 98507 ms.
---------------------------------------------------------